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  TEL/WhatsApp: +86 17622605414
Mail: admin@transformercoilwindingmachine.com
    Web:www.transformercoilwindingmachine.com

KX-AM-080 Fully Automatic Single Station Toroidal CMC Hook Machine
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	设备型号Device model
	GW-AM-080 Fully Automatic Single Station Toroidal Hook Machine

	磁环最小最大加工尺寸

Minimum and maximum processing dimensions of magnetic core
	内径:最小4mm  外径最大:25mm

Inner diameter: minimum 4mm Maximum outer diameter: 25mm

	主轴最大转速

spindle maximum speed
	3000rpm

	AC伺服马达

AC servo motor
	绕线主轴：400W 

Winding spindle: 400W

	排线电机/上下料电机

Wiring motor/loading and unloading motor
	57步进/42步进

57 steps/42 steps

	排线角度

wire arrangement angle
	360度1圈，设定单位0.1度

360 degrees per circle, setting unit is 0.1 degrees

	轴停精度 Axis stopping accuracy
	正负1度 plus or minus 1 degree

	适用磁环规格

Applicable magnetic core specifications
	最大外径:25；最小内径:2； 最大厚度:12

Maximum outer diameter: 25; Minimum inner diameter: 2;  Maximum thickness: 12

	适用线径 Applicable wire diameter
	0.25mm-1.5mm

	排线方式 wire arrangement
	正反排（可自动抽线头）

Front and back arrangement (can automatically pull out wire ends)

	轴移动量 Axis movement amount
	XB:150mm / YB:120度 ZB/30mm

XB:150mm / YB:120 degree ZB/30mm

	轴移动速度Axis moving speed
	300mm/sec

	控制方式 control method
	CNC 5轴控制板卡（自主研发）

CNC 5-axis control board (independent research and development)

	储存方式 Storage method
	RAM+FLASH储存，无资料丢失故障

RAM+FLASH storage, no data loss failure

	电源电压voltage
	单相三线制Single phase three wire system

	
	220V,50HZ

	消耗电力consume electricity
	1.0KW


	压缩空气压力compressed air pressure
	0.5-0.8MPa

	设备尺寸Equipment size
	1500mm(L)×800mm(W) ×1500mm(H)

	设备重量equipment weight
	200Kg


GW-AM-080 machine is a high-tech automatic loading and unloading winding and soldering machine, man-machine dialogue display screen and the nose and fixture of flexible replacement system combined with machine, by precision accessories and independently developed PLC system, powerful servo motor drive head, precision servo motor drive iron core.

The user can use the machine through the simple setting of the operation technician. GW-AM-080 is suitable for special single wire and double wire winding specifications, precision winding, maintenance free, simple repair. 

This equipment is applicable to all kinds of ring coil material application manufacturing, the main components of the equipment are developed and produced by the company, self-assembled, to ensure excellent quality and processing characteristics, the best production quality guarantee and a strong publicity effect for customers, improve your competitiveness in the domestic and international markets.

1. The key parts of the machine are imported from Taiwan or Japan, with strong reliability and high durability, which greatly increases the service life of the equipment;

机器关键零部件采用台湾或日本进口,可靠性强,耐用度高,大大增长设备使用寿命;

2. Novel appearance design, simple and reliable structure, simple operation and convenient maintenance;

外观设计新颖,结构简单可靠,操作简单维护方便;

3. The equipment adopts self-developed CNC high-speed motion control board, touch screen human-machine dialogue debugging parameters, and easy-to-understand Chinese and English displays;

设备采用自主研发CNC高速运动控制板卡,触摸屏人机对话调试参数,中英文显示易于理解;

4. The equipment has the functions of automatic thread hanging, automatic thread cutting, automatic alarm and shutdown when disconnected, and a single person can take care of more than 8 pieces of equipment;

设备具有自动挂线,自动切线,断线自动报警停机功能,单人可以看管8台以上设备;

5. The standardized design of the equipment comes with built-in plug-in module extension functions and has secondary development function modules;

设备标准化设计自带机构外挂模块扩展功能,具备二次开发功能模块;

The equipment wiring arrangement has high precision, the controller human-machine interface display, Chinese and English layouts can be switched between each other, 10 sets of programs can be stored, the computer can store unlimited, 20 threads and 200 lines of programmable programs, real-time display of operating parameters, such as Storage/winding, speed, number of turns, output, and product time cycle, etc. The program can set acceleration and deceleration to avoid impact breakage, the number of turns is accurate, and copper wire is saved. It can be completed automatically: dense winding, sparse winding , forward and reverse winding, segmented winding, multi-wire parallel winding and other winding methods, suitable for winding various conventional and special-shaped inductor coils in the inductor coil, resistor coil, and transformer coil industries.

设备排线整列精度高,控制器人机界面显示,中、英版面可互相切换，可存储10组程序，电脑可无限储，20个线程200行可编程程序,实时显示运行参数，如储/绕线、速度、圈数、产量、及产品时间周期等、程序可设加速度和减速度,可避免冲击断线,圈数准确, 铜线更节省可全自动完成:密绕、疏绕、正反绕、分段绕、多线并绕等绕线方式，适用电感线圈、调阻器线圈、变压器线圈行业的各种常规及异形电感线圈绕线。
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Packaging 

Packaging Material: Carton/Wooden case with foam inside. 

General package(Paper carton or plastic bag): For small equipped parts for Digital CNC Wire Coil Winding Machine, Package it with form and pack paper to guarantee unbroken during the transport.

2.Wooden case package: For larger scale Digital CNC Wire Coil Winding Machine ,we have special skilled carpenter, who would make the proper wooden case with exact thickness, density,length. The up arrow ↑marked on the outer wooden case. Buffer material would be put in the wooden case to prevent crack and shock.
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FACTORY:

Founded in 1993,KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD. has established itself as a well-known manufacturer specializing in high-performance winding machines, along with associated production equipment and technical expertise. A standout offering in its advanced product lineup is the GW-AM-080 Fully Automatic Single Station Toroidal CMC Hook Machine—a precision-engineered solution designed for automated toroidal coil winding with CMC hook technology, enhancing the company's capabilities in specialized toroidal component manufacturing.

Beyond delivering specialized equipment like the GW-AM-080 Fully Automatic Automatic Single Station Toroidal CMC Hook Machine, KIOXIA LIGHT RING provides highly cost-effective comprehensive manufacturing solutions. These solutions cater to the production needs of various wound components, including transformers, chokes, and toroidal coils, ensuring reliable support for efficient, high-quality processing across diverse electronic component manufacturing applications.
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KIOXIA LIGHT RING EQUIPMENT GROUP CO.,LTD.
Add: Building G, No.209 Zhonghuan East Road, Free Trade Zone (Airport Economic Zone), Tianjin

